# Factory Mode User Help

## Getting Started

Factory mode is entered via a bluetooth serial connection to the CPF. In order to access this interface, we will assume you have a bluetooth RS232 module hooked up to your PC. Open the serial port using baudrate 115200 kbps 8N1 with no flow control. After powering the float you should see a message:

    Press $$$<CR> to enter factory mode. You have 5 seconds...

Enter the `$$$` followed by the enter key on your keyboard. You can do this multiple times to be sure, the CPF will wait 5 seconds irregardless. Upon success, you will be welcomed with the factory mode prompt:

    CPF>


## Command Descriptions

### General Commands
#### `help`
#### `cd`
#### `dir`
#### `rm`
