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1.0 INTRODUCTION.
The Monterey Aquarium Research Institute (MBARI) is developing a deep ocean underwater science observatory. The maximum working depth of the observatory is planned to be 4000 meters. The observatory design includes a series of seafloor placed science instruments connected together with ROV laid electro-optical cable referred to as the Benthic Cable.
It is MBARI’s intention that the cable vendor, not MBARI or its independent contractors, design the cable described in this document. Section 2.0, Performance Requirements, represents MBARI’s only firm requirements.   Items indicated as To Be Determined (TBD) are open to further discussion between MBARI and the vendor.

2.0 PERFORMANCE REQUIREMENTS.


2.1 General and Environmental. The benthic cable performance shall not be degraded by conditions typical of the working environment, including:

2.1.1 Continuous submergence in seawater over working life.

2.1.2 Temperatures from 0 to 25 degrees Centigrade. 

2.1.3 Hydrostatic pressure equivalent to 4000 meters seawater (vendor to advise on cable suitability for 6000 meter operation).

2.1.4 Materials Compatibility  TBD

2.1.5 Storage Conditions.  TBD

2.1.6 Service Life.  The Benthic cable shall provide a minimum of three years of service while continuously submerged in a dynamic ocean environment.


2.2 Mechanical
2.2.1 Diameter – Per Manufacturer Spec

2.2.2 Weights – Per Manufacturer Spec

2.2.3 Working Strength - Per Manufacturer Spec

2.2.4 Breaking Strength - Per Manufacturer Spec

2.2.5 Fatigue Life - Per Manufacturer Spec

2.2.6 Elongation - Per Manufacturer Spec

2.2.7 Rotation - Per Manufacturer Spec 

2.2.8 Minimum - Per Manufacturer Spec 

2.2.9 Packaging – The cable is intended to be packaged in a self deploying cable pack.  This will require the cable to withstand one 360 degree twist (around the cable axis) as the cable is wound around one revolution on a mandrel of the minimum bend diameter specified by the cable vendor.  Winding will be done at minimum tension.

2.3 Optical

2.3.1  Fiber Count.  There shall nominally be four single-mode optical fibers.  Fibers shall be Corning SMF 28.  Use of alternate fiber shall be by written agreement between vendor and MBARI. . The optical specifications must be met over the specified cable service life during continuous operation under the conditions described in the “General and Environmental” and the “Mechanical” sections above.

2.3.2 Optical Attenuation. N/A

2.3.3 Optical Attenuation Uniformity. No single point attenuation discontinuity in any fiber in the finished cable shall be greater than 0.15 dB at either 1310 Nm. or 1550nm. wavelengths, as measured with an OTDR.

2.3.4 Optical Dispersion. Individual fiber specifications for optical dispersion in the completed cable shall meet the pre-cabled fiber manufacturer’s specifications for the fiber used, as measured by EIA/TIA 455-175.

2.3.5 Fiber Proof Test. Individual fibers will be proof tested at the time of manufacture to a minimum of 100kpsi.

2.3.6 Fiber Identification.  Fibers or their over-jacketing shall be color coded or otherwise indelibly marked at least every meter for identification.  

2.4  Electrical


2.4.1 General.  The cable will be used for electrical power transmission while submerged in the marine environment.  The cable shall provide a minimum of two electrical conductors insulated from one another, and from seawater.


2.4.2 Working Voltage.  The cable will be used at a working voltage between conductors, or between conductors and seawater, of up to 425 Volts DC.   At this voltage, the maximum electrical stress present at any point in the cable insulation system shall be less than or equal to 2.0 kV/mm (51 volts/mil).  The insulation system used must be suitable for continuous high DC electric field stress.


2.4.3 Insulation Resistance.  The Insulation Resistance of each conductor in the as-built cable shall be a minimum of 3,000 Megohms per kilometer, measured at the working voltage of Section 2.4.2 above.  The resistance shall be measured between the test conductor, and the other conductor(s) plus the cable armor plus any other metallic cable elements, tied together.


2.4.4 Conductor Resistance.  Per SB-43899

2.4.5 Production Testing.   Each individually insulated conductor shall be tested for insulation resistance, before cable assembly, in a water bath. Impulse testing may be substituted for wet testing at manufacturer’s discretion.
The test conditions and criteria for acceptance shall be as specified in Section 2.4.3 above.  The completed cable shall be evaluated for Partial Discharge at the working voltage of Section 2.4.2 above.  No detectable discharge is permitted, within the detection limits of the test equipment employed.  Optical attenuation at 1310 and 1550 nm (nominal values) shall be tested.  

2.4.6 Conductor Identification.   The individual conductors shall be color coded or otherwise made visually distinguishable from one another, either throughout their length, or at regular increments not to exceed 0.33 meter.

3.0 DOCUMENTATION

Vendor shall provide copies of all incoming inspection, in-process production and final inspection tests done during cable manufacture.

4.0 QUALIFICATION TESTS. 

The following tests may be performed by MBARI or an independent test contractor at MBARI expense prior to final acceptance of the completed cable.


4.1 Electrical. A benthic cable specimen will be subjected to conductor resistance and insulation resistance tests to obtain the as delivered values.
4.2 Optical Static Attenuation. The benthic cable will be tested for optical attenuation at 1310Nm and 1550Nm wavelengths to obtain the as delivered values.
4.3 Optical Characterization. The optical attenuation in response to tensile loading will be measured.
4.4 Mechanical Characterization. A benthic cable section will be tested for tension induced changes in elongation, diameter, torque and rotation. The benthic cable will also be tested for yield and breaking strength.
4.5 Suitability for packaging.  The benthic cable is intended to be packaged on a 20” diameter spool. 
5.0 DELIVERY.

Delivery shall be quoted FOB Moss Landing, California, 95039.

Cable shall be delivered suitably packaged for transportation and storage.

