**********************************************************
GHI Electronics, LLC
FEZ Config for NETMF 
**********************************************************

SDK Version 2013 R3 (v1.0.0)
October 23, 2013
======================================

Release Info

•	Initial release.

Known Issues

•	When setting the display configuration on G120, sometimes the device remains in Loader mode and does not start the firmware. To fix this, goto Advanced > Reboot CLR and the device will function properly again. 
•	Setting the display configuration on Hydra can sometimes fail.