ARGO+ISUS Assembly Procedure
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Version 2
1. Webb’s shop manufactures modified parts (Top endcap, CTD chassis)                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                          

2. Seabird assembles and calibrates CTD (as previously)
3. CTD sent to Monterey (or Satlantic)
4. MBARI (or Satlantic) adds and calibrates ISUS.

5. CTD+ISUS sent to Webb
6. Webb assembles float
7. Float sent to Seattle
8. UW measures current consumption in 2-gallon bomb 
9. UW installs Li batteries

10. UW ballasts float in large FW pressure vessel (w/probe dummy)
11. UW checks Iridium communication

12. UW checks ISUS calibration

13. Float sent to sea
Version 1
1. Shops manufactures modified parts (Bottom endcap, Main chassis)
2. Seabird assembles and calibrates CTD

3. CTD sent to Webb                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                  
4. Webb assembles ISUS version of APEX float

5. Float sent to Monterey

6. MBARI adds ISUS, but fixes probe inside housing.

7. Float sent to UW (with plug and probe dummy)
8. UW configures APEX controller, Iridium modem, etc

9. UW measures current consumption in 2-gallon bomb (w/plug)

10. UW rights float in SW pool (w/probe dummy)

11. UW checks Iridium communication

12. Float sent to Monterey

13. MBARI installs ISUS probe, and calibrates ISUS
14. MBARI seals float, adds desiccant, and pulls 5” vacuum.

15. Float sent to UW

16. UW installs Li batteries

17. UW ballasts float in large FW pressure vessel

18. UW checks Iridium communication

19. UW checks ISUS calibration

20. Float sent to sea
