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Model name: DFassy
Current Configuration: FullAssy

	Solid Bodies

	Document Name and Reference
	Treated As
	Volumetric Properties
	Document Path/Date Modified

	Cut-Extrude8
[image: ]
	Solid Body
	Mass:0.000124513 lb
Volume:0.000926478 in^3
Density:0.134394 lb/in^3
Weight:0.000124428 lbf

	C:\Users\jon\Desktop\Temp_DuraFet\DurFETpcb.SLDPRT
Jun 29 12:27:50 2016

	Cut-Extrude7
[image: ]
	Solid Body
	Mass:0.000184119 lb
Volume:0.00137 in^3
Density:0.134394 lb/in^3
Weight:0.000183994 lbf

	C:\Users\jon\Desktop\Temp_DuraFet\DurFETpcb.SLDPRT
Jun 29 12:27:50 2016

	BottomWires
[image: ]
	Solid Body
	Mass:0.000165465 lb
Volume:0.0012312 in^3
Density:0.134394 lb/in^3
Weight:0.000165352 lbf

	C:\Users\jon\Desktop\Temp_DuraFet\DurFETpcb.SLDPRT
Jun 29 12:27:50 2016

	Cut-Extrude1
[image: ]
	Solid Body
	Mass:1.08693e-005 lb
Volume:0.000261545 in^3
Density:0.041558 lb/in^3
Weight:1.08619e-005 lbf

	C:\Users\jon\Desktop\Temp_DuraFet\Epoxy_Bottom.SLDPRT
Jun 30 17:31:57 2016

	Boss-Extrude2
[image: ]
	Solid Body
	Mass:1.44967e-005 lb
Volume:0.00034883 in^3
Density:0.041558 lb/in^3
Weight:1.44869e-005 lbf

	C:\Users\jon\Desktop\Temp_DuraFet\Epoxy_Middle.SLDPRT
Jul 06 12:23:37 2016

	Split Line1
[image: ]
	Solid Body
	Mass:3.41024e-005 lb
Volume:0.00040513 in^3
Density:0.0841766 lb/in^3
Weight:3.40793e-005 lbf

	C:\Users\jon\Desktop\Temp_DuraFet\ISFET Die.SLDPRT
Jul 06 12:27:00 2016
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	Study name
	Static 1

	Analysis type
	Static

	Mesh type
	Solid Mesh

	Thermal Effect: 
	On

	Thermal option
	Include temperature loads

	Zero strain temperature
	298 Kelvin

	Include fluid pressure effects from SOLIDWORKS Flow Simulation
	Off

	Solver type
	FFEPlus

	Inplane Effect: 
	Off

	Soft Spring: 
	Off

	Inertial Relief: 
	Off

	Incompatible bonding options
	Automatic

	Large displacement
	Off

	Compute free body forces
	On

	Friction
	Off

	Use Adaptive Method: 
	Off

	Result folder
	SOLIDWORKS document (C:\Users\jon\Desktop\Temp_DuraFet)
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	Unit system:
	English (IPS)

	Length/Displacement
	in

	Temperature
	Fahrenheit

	Angular velocity
	Hertz

	Pressure/Stress
	psi
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	Model Reference
	Properties
	Components

	
		Name:
	CoorsTek AD-96

	Model type:
	Linear Elastic Isotropic

	Default failure criterion:
	Unknown

	Tensile strength:
	32053.3 psi

	Compressive strength:
	299938 psi

	Elastic modulus:
	4.4e+007 psi

	Poisson's ratio:
	0.21  

	Mass density:
	0.134394 lb/in^3

	Thermal expansion coefficient:
	4.44444e-006 /Fahrenheit



	SolidBody 1(Cut-Extrude8)(DurFETpcb-1),
SolidBody 1(Cut-Extrude7)(DurFETpcb-2),
SolidBody 1(BottomWires)(DurFETpcb-3)

	Curve Data:N/A

	
		Name:
	3M_2214_Non-Filled Epoxy

	Model type:
	Linear Elastic Isotropic

	Default failure criterion:
	Unknown

	Tensile strength:
	9000 psi

	Elastic modulus:
	700000 psi

	Poisson's ratio:
	0.394  

	Mass density:
	0.041558 lb/in^3

	Shear modulus:
	46252.5 psi

	Thermal expansion coefficient:
	0.00013 /Fahrenheit



	SolidBody 1(Cut-Extrude1)(Epoxy_Bottom-1),
SolidBody 1(Boss-Extrude2)(Epoxy_Middle-1)

	Curve Data:N/A

	
		Name:
	Silicon

	Model type:
	Linear Elastic Isotropic

	Default failure criterion:
	Unknown

	Yield strength:
	17404.5 psi

	Elastic modulus:
	1.63022e+007 psi

	Poisson's ratio:
	0.28  

	Mass density:
	0.0841766 lb/in^3

	Shear modulus:
	7.10685e+006 psi



	SolidBody 1(Split Line1)(ISFET Die-1)

	Curve Data:N/A
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	Fixture name
	Fixture Image
	Fixture Details

	Fixed-1
	[image: ]
		Entities:
	1 face(s)

	Type:
	Fixed Geometry




	Resultant Forces
	Components
	X
	Y
	Z
	Resultant

	Reaction force(lbf)
	-8.52237e-005
	204.378
	-0.000174896
	204.378

	Reaction Moment(lbf.in)
	0
	0
	0
	0


 



	Load name
	Load Image
	Load Details

	Pressure-1
	[image: ]
		Entities:
	10 face(s)

	Type:
	Normal to selected face

	Value:
	3000

	Units:
	psi

	Phase Angle:
	0

	Units:
	deg
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	Contact
	Contact Image
	Contact Properties

	Contact Set-1
	[image: ]
		Type:
	Bonded contact pair 

	Entites:
	2 face(s)




	Contact Set-2
	[image: ]
		Type:
	Bonded contact pair 

	Entites:
	2 face(s)




	Global Contact
	[image: ]
		Type:
	Bonded

	Components:
	1 component(s)

	Options:
	Compatible mesh
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	Mesh type
	Solid Mesh

	Mesher Used: 
	Standard mesh

	Automatic Transition: 
	Off

	Include Mesh Auto Loops: 
	Off

	Jacobian points
	4 Points

	Element Size
	0.008 in

	Tolerance
	0.0004 in

	Mesh Quality
	High
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Reaction forces
	Selection set
	Units
	Sum X
	Sum Y
	Sum Z
	Resultant

	Entire Model
	lbf
	-8.52237e-005
	204.378
	-0.000174896
	204.378


Reaction Moments
	Selection set
	Units
	Sum X
	Sum Y
	Sum Z
	Resultant

	Entire Model
	lbf.in
	0
	0
	0
	0
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	Name
	Type
	Min
	Max

	Stress1
	VON: von Mises Stress
	0 psi
Node: 1789604
	26038.1 psi
Node: 2402830

	[image: ]
DFassy-Static 1-Stress-Stress1



	Name
	Type
	Min
	Max

	Stress2
	VON: von Mises Stress
	0 psi
Node: 1789604
	26038.1 psi
Node: 2402830

	[image: ]
DFassy-Static 1-Stress-Stress2



	Name
	Type
	Min
	Max

	Stress3
	VON: von Mises Stress
	0 psi
Node: 1789604
	26038.1 psi
Node: 2402830

	[image: ]
DFassy-Static 1-Stress-Stress3



	Name
	Type
	Min
	Max

	Stress4
	VON: von Mises Stress
	0 psi
Node: 1789604
	26038.1 psi
Node: 2402830

	[image: ]
DFassy-Static 1-Stress-Stress4



	Name
	Type
	Min
	Max

	Displacement1
	URES:   Resultant Displacement
	0 in
Node: 1515005
	0.000122687 in
Node: 2524983

	[image: ]
DFassy-Static 1-Displacement-Displacement1



	Name
	Type
	Min
	Max

	Displacement2
	UY: Y Displacement
	-0.000120886 in
Node: 2524983
	0 in
Node: 1515005
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DFassy-Static 1-Displacement-Displacement2



	Name
	Type
	Min
	Max

	Strain1
	ESTRN: Equivalent Strain
	1.034e-005 
Element: 522125
	0.0324084 
Element: 1477912
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DFassy-Static 1-Strain-Strain1



	Name
	Type
	Min
	Max

	Stress5
	P1: 1st Principal Stress
	-10405.1 psi
Node: 2402826
	19764.2 psi
Node: 2402734

	[image: ]
DFassy-Static 1-Stress-Stress5



	Name
	Type
	Min
	Max

	Stress6
	P2: 2nd Principal Stress
	-14534.3 psi
Node: 2402826
	10288.8 psi
Node: 176737

	[image: ]
DFassy-Static 1-Stress-Stress6



	Name
	Type
	Min
	Max

	Stress7
	P3: 3rd Principal Stress
	-30736 psi
Node: 2402821
	3800.56 psi
Node: 176720

	[image: ]
DFassy-Static 1-Stress-Stress7



	Name
	Type
	Min
	Max

	Stress8
	P1: 1st Principal Stress
	-10405.1 psi
Node: 2402826
	19764.2 psi
Node: 2402734

	[image: ]
DFassy-Static 1-Stress-Stress8



	Name
	Type
	Min
	Max

	Stress9
	P1: 1st Principal Stress
	-10405.1 psi
Node: 2402826
	19764.2 psi
Node: 2402734
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DFassy-Static 1-Stress-Stress9
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	Image-1
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	Image-2
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	Image-3
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	Image-4
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	Image-5
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	Image-6
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	Image-7




	[image: ]

	Image-8
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	Image-10
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	Image-11
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	Image-12
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	Image-13
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	Image-14
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	Image-15
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	Image-16
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	Image-17
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	Image-18
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