SURpH Sensor Assemby Instruction
SURpH Version Number: 3.2
SURpH Serial Number: SURpH009
ISFET CCA Assembly: uncoated
Step 1 Insert Helicoils
1.1 Inspect 2X 0-80 and 1X 2-56 STI tapped holes, chase if necessary
1.2 Install all 3 helicoils (BOM x, y).  Ensure helicoil is ~0.005” below surface
1.3 Remove tangs if necessary

Step 2 [bookmark: _GoBack]Install Van London Pellet
