Circuit Components:

RTC Plug
[image: http://cdn.shopify.com/s/files/1/0032/7122/products/DSC_0697_large.jpg?v=1256718790]
	Is a clock
	Can keep time when powered off due to internal battery
	http://www.digitalsmarties.net/products/rtc-plug
	
Relay Plug
[image: http://files.jeelabs.org/2010/08/dsc_1812.jpg]
[image: http://jeelabs.net/attachments/download/274/pinout.png]
Normal relay switch. 

Memory Plug
[image: Memory Plug]
Ours has 2 memory blocks so 256 Kbyte of memory 
3.3 V
UART Board
[image: UARTPlug1.jpg]
[image: http://jeelabs.net/attachments/download/238/up1._0000020e.png]
Allows to change voltage types.
Used to convert signal from the CO2 sensor so it is readable by the jeenode. 

Carbon Dioxide Sensor
General Electric T6615 module
[image: Amphenol Advanced Sensors T6615-5K]
Infrared CO2 sensor
Readings are affected by humidity 
Accuracy within 10% or 75 ppm 

Air Pump
Thomas 
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UART Plug connector:

TS | AXD | TXD [ PWR | CTs [ GND A

Port connector: nun
71717
PWR | DIO | GND | +3v | AIO | iRG TG
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Relay Plug connector: Relay Plug
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