I2C BUS POWER BOARD SPECIFICATION READ-ME
File Name:  10020174_i2CPWR_REV1.brd
QTY: 10 MIN
Turn Time: 4 Days 

Layers: 2 

Layer Orientation:

1. TOP

2. BOT

Thickness:  0.062 "" FR4 

Dimensions: 3.00” x 4.00" 

Finish: SMOBC/HASL 

Cu Weight: 1oz (ALL LAYERS)
Trace width/space: 0.005”/0.007”
Smallest hole size: 0.016" 

Sides to solder mask: Both Sides (BLACK)

Sides to silk screen:  Both Sides (WHITE) 

IPC-356 FILE (10020174_i2.ipc) INCLUDED FOR TEST
