SuperDriodrobot

RS-232 transceiver

As shipped pinout and configuration

	DB9S
	Function
	MAXpin
	Function
	Function
	MAXpin
	PCBpoint
	Wire Color
	Connector/

Pin

	2
	TX(o)
	14
	Dout1
	Din1
	11
	4
	BLK
	WHT/4

	3
	RX(i)
	13
	Rin1
	Rout1
	12
	3
	GRN
	WHT/3

	7
	RTS(i)
	8
	Rin2
	Rout2
	9
	6
	BLU
	BLK/1

	8
	CTS(o)
	7
	Dout2
	Din2
	10
	5
	BRN
	BLK/2

	5
	SigGnd
	15
	GND
	GND
	15
	2
	WHT
	WHT/1

	
	
	
	
	VCC
	16
	1
	RED
	WHT/2


The DB9 connector should be pinned to plug directly into a standard IBM PC serial port.

What we need

	Function
	Wire Color
	4-Pin Connector
	2-Pin Connector

	TX
	BLK
	2
	

	RX
	GRN
	3
	

	RTS
	BLU
	
	1

	CTS
	BRN
	
	2

	SigGnd
	WHT
	4
	

	VCC
	RED
	1
	


4 pin connector used for just Data with the Dwarf debug port while the 4 and 2 pin are used to talk to sleepy using handshaking.

