Dwarf Core Features
2 servo Channels
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Bus 
Samtec ESQ-125-49-G-D


Power


Housing Molex 39-01-4040
Contacts Molex 39-00-0163

I2C
Amp 746285-2

Servo Amp connector system

Interim Clip 104500-2
Housings 103648 series

Contacts 104479-7


Serial


Housing Molex 50-57-9406 
Contacts Molex 16-02-0103
