Dwarf Rvalve Features
Daughter card to Core

4 Rotary valve


Per Channel



Full H-bridge



2 A



Absolute Serial Encoder reader


Current monitoring

8 Solenoids


H-Bridge control


Latching


Non-Latching


1.5 amp 

