PC-104 CARRIER BOARD_2P9 README_FAB.TXT

Design Contact: John Zsori - Corporate Engineering Services
Voice:   408.293.9360
Fax:     408.293.9360
Cell:    408.391.6656
email:   john_zsori@pacbell.net

REFER ALL PCB DESIGN RELATED ISSUES TO JOHN ZSORI

Client: MBARI
7700 Sandholdt Road
Moss Landing, CA  95039
Wayne Radochonski - 831.775.1700


Fabrication data included in PC-104 CARRIER BOARD_2P9-CAM.ZIP:

                PowerPCB Gerber Files (RS-274-X Format)
      
PC-104 CARRIER BOARD_2P9-Ln.PHO     PCB Copper Layer 
                (where n = layer number, 1=Primary (Top) Side)
PC-104 CARRIER BOARD_2P9-ST.PHO     Primary Silkscreen (Top)
PC-104 CARRIER BOARD_2P9-SB.PHO     Secondary Silkscreen (Bottom)  
PC-104 CARRIER BOARD_2P9-MT.PHO     Primary Solder Mask (Top)
PC-104 CARRIER BOARD_2P9-MB.PHO     Secondary Solder Mask (Bottom)
PC-104 CARRIER BOARD_2P9-PT.PHO      Primary Paste Mask (Top)
PC-104 CARRIER BOARD_2P9-PB.PHO    Secondary Paste Mask (Bottom)
PC-104 CARRIER BOARD_2P9-DD.PHO     Drill Drawing

	Fabrication Drawings

PC-104 CARRIER BOARD_2P9-DD.PDF     Drill Drawing in Adobe format

	Drill Files

PC-104 CARRIER BOARD_2P9-NC.DRL     NC Drill
PC-104 CARRIER BOARD_2P9-NC.REP     NC Drill Report (Sizes & Quantities)
PC-104 CARRIER BOARD_2P9-NC.LST     NC Drill Sizes & Coordinates


                Netlist

PC-104 CARRIER BOARD_2P9-IPC.NET    IPC-D-356 Format Netlist (See Note 2)
PC-104 CARRIER BOARD_2P9.tgz            PADS format ODB++ file

Notes:

1. The soldermask Gerber data is 1:1 scale. Adjust the soldermask size
to your specific manufacturing tolerances while maintaining maximum web.

2. Compare the provided IPC-D-356 netlist with the Gerber generated netlist 
as a verification check for possible connectivity errors.

3. Regardless of CAD data vendor to insure the all vias under BGA are covered with soldermask.
Vendor may encroach vias to preclude entrapment.