ea_i2s
------

An example that illustrates usage of the external
UDa1380 audio codec. At startup a short audio clip 
will be played. After startup it can be play again by
moving the joystick to the UP position.

Moving the joystick left or right will play the 
sound in the left or right audio channel.
