Sleepy Requirements

What does Sleepy have to do?

1) Manage power to system

A) Camera Power – regulated

a) 12V

b) 0.75A

B) System Raw power – unregulated

a) 10 – 16V

b) ?A

C) 3.3V – regulated

a) 3.3V

b) 0.5A

c) Isolated from input, common tie on secondary

D) 5V – regulated

a) 5V

b) 1A

c) Isolated from input, common tie on secondary

2) Provide I2C bridge to Snow White

A) Bus termination

B) ESP protocol

C) RS-232 to Snow White

3) Manage Modem power and communications

A) control power to modem

B) Communications for modem

a) RS-232 level translators

b) Communications switch – low level

c) Fault Isolation

d) Tx, Rx, Handshake in and out

4) Environmetal monitoring

A) Humidity

B) Temperature

C) Water Sense

D) Pressure

5) Reset

A) Sleepy reset from contact closure

B) Reset control of Mom

