To: 
Bob Rossi

PhotoFabrication Engineering Inc.


500 Fortune Blvd


Miloford, MA 01757

From : Scott Jensen


Monterey Bay aquarium Research Center


7700 Sandholdt Rd.


Moss Landing, CA 95046

Bob,

   Enclosed are four frits from two different fabrication runs from your company.  As per our phone conversation of January 24, 2008, please examine and measure these items.  In our application the exact shape and size of the hole is not as critical as the amount of remaining web material.  The frits are used to support a fine porosity filter membrane and must be strong enough to support the media at our maximum system pressure.  The flow rate through the frits is small and pressure drop is not going to be determined by the final diameter of the frit holes but instead buy the fine porosity of the filter media.  Based upon calculations of stress in our application we would like to control the diameter of the holes to 0.0265 +/- 0.003.  The two frits with the larger diameter holes are not acceptable to us while the smaller diameter holes are acceptable.  Since the actual hole is not easily measurable by a pin gauge we used the mass of the frit to determine the effective size of the holes. Using the frit’s mass as a measurement of acceptance we calculate that each frit should measure between 0.47 and 0.62 grams.  The frit mass specification will not be used to determine the number of frits in a lot but instead as an individual frit quality parameter.
I look forward to hearing from you,

Scott Jensen

