MBARI
Regular user maintenance schedule

Lubrication:

Ballscrews for syringes and clamps need to be lubricated with LubriFilm.

Syringe plungers need to be lubricated with CST 1000 lube.

Cleaning:

Flush Puck Garage needs to be disassembled and all parts cleaned. 

Heater pads need to be cleaned of any residue buildup.

Waste containers need to be emptied.

Check & Replace:

Check and replace as necessary, clamp and heater O-rings.
 Air filters may need to be replaced if they get wet.

Calibration:

Check thermal and pressure calibrations annually.

Software:

Install patches as received.

