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ISMS:	ON hold until ISMS is determined to be going.	
                Change Igo power supply from 24 to 48V
                Incorporate power switching 
                Drawings
                Fabrication
ISUS:
                Select and procure power supply
                Incorporate power switching
                Drawings 
                                Modify and include
                Fabrication          
Battery Combiner:
                Power question needs answering first


ISMS?

Ambient valves, flush/tox?
Wand?
ORDER:

New filters for DWSM
Open issues:
	Compliance bags  testing options
	Sphere valves
New IEP Pump:
                Servo controller selection
                Drawing changes
                Installation
                Testing
Sphere heating
WebRelay:
                Change to quad to support ISUS and ISMS
                Drawings
                Fabrication
HPP encoder failure:
                In house failure analysis – inconclusive
                Sent to Manufacturer
                Order more spares
                Install spares
HPP drive methodology


In trailer work
	Flush, empty DWSM
	Flush HPI
	Remove sample compliance bag
	Filter oil
	Replace bags   Sample only
	Test switch points   Sample only
	New compliance bags
	Review how HPI works on current drive (torque mode)
	Test FMI IEP in bucket
	Install FMI IEP in Resampler
	Test FMI IEP under pressure

	Fix Gordon

Heater status/control?
	Full cycle test Under HP
Inhale-decomp-Sample 
Core process, develop array, PCR?
Recompress, Empty 
	CTD/ISUS in a bucket, yes.
Chill Down to 4C
Full cycle cold test.

Elevator and Foam pack to High Bay
Inspect sphere vent ports
Remount Batteries
Plug 4 ports on Battery Combiner box
Install ISMS?
Install CTD
Add foam to pack
	Remove Ac. Modem
Install Pinger, Strobe, etc.
Attach bumper rings

Canning Gordon
	Add hobo’s
Load reagents
Load Pucks
Empty wastes
Install sphere insulation

Can Sphere
Torqe bolts, cross pattern  (120 in-lbs)
Go-no go gauge test
Leak test and N2 purge.
Clean and reset sphere relief (5 turns out, 4 psi)

Can DWSM
Leak test DWSM bells

	Attach foam pack
Attach R2D2
Change out CTD
	CTD batts
Manual Weight Release only?

Test Tank?
	Weigh, trim and balance
	Post Can QC
Fluidic Stream (Sample point/DWSM/ISMS/ISUS/CTD…)
	Curves?
	Other?
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