Lung Style:

Transfer pump: 

1. Metering to 1% accuracy

2. 75 psig max (and target)

3. 20 W max power

4. Fluid, oil, (Tellus 15?)

5. Bi-directional

6. Minimum inhalation flow rate, 4-lpm

7. 100:1 turn down possible on motor on motor

8. Full torque capable at low speeds.

9. Servo channel control

De-Pressure Pump

1. 20 W max power

2. Run from solenoid switch (source) (+,-, off)

3. Preferred to turn on an pump until pressure met.

