DWSM ETHERNET DISCONNECT
File Name:  10020314_ETHERNET-DISCONNECT_REV0-0.brd
QTY: 10 MIN
Turn Time: 3 Days 

Layers: 2 

Layer Orientation:

1. TOP

2. BOT

Thickness:  0.062" FR4 

Dimensions: 2.80” x 1.60" 

Finish: SMOBC/HASL 

Cu Weight: 1oz (ALL LAYERS)
Trace width/space: 0.005”/0.007”
Smallest hole size: 0.038" 

Sides to solder mask: Both Sides (BLACK)

Sides to silk screen:  Both Sides (WHITE) 

IPC-356 FILE (10020314_ETHERNET-DISCONNECT_REV0-0.ipc) INCLUDED FOR TEST
