ESP DWSM

December 4, 2006

Friday: Mobilization
· Tool sled moved to dock and attached to ROV

· Power and Communication cable

· Strap down cables

· Finalize Plumbing

· Locate Cameras

· Get buckets for purging

· Communication infrastructure

· Laptop

· Instrument connected directly or with network

· Operators location

· Instrument Check out

· Initial Communications

· Homing

· Purge

Monday: Dive Day

· Arrive at Dock at  6:30 AM
· Depart Dock at 7:00 AM
· Site 1000 meters of water without risk of hitting bottom. Robi midwater
· Transit time 1:30
· In transit Prepare instrument

· Fill Buckets for purging
· Run DWSM.deckprep
· Run DWSM.diveprep
· If bubble  greater than 40mL run DWSM.purge until bubble reported less than 40mL

· Instrument ready to dive

· Vehicle overboard

· Monitor Pressure   DPU.status.pressure
· Dive to 10meters and hold

· Run DWSM.diveprep
· Monitor Pressure   DPU.status.pressure
· Dive to 200 meters

· Monitor Pressure for 20 minutes  Piston
· For the following table of depths repeat this process

· Dive to (Depth from table)

· Run DWSM.sample (Volume from table)

· DWSM.exhale

	Sample
	Depth
	Volume (ml)
	Start
	Finish

	1
	10
	500
	
	

	2
	200
	500
	
	

	3
	500
	500
	
	

	4
	750
	500
	
	

	5
	1000
	1800
	
	

	6
	900
	
	
	

	7
	600
	
	
	

	8
	10
	
	
	

	9
	
	
	
	


· Vehicle onboard
· Return to Dock

· In Transit

· DWSM.rinse

· When do we remove DWSM from Ship and ROV

