Pull mooring only onto deck
Mooring lift line
	Lifting Line
	Float
	Screw Pin Shackle
	3 tie wraps
	Dive Bag
	2 Bale and hairpin cotter pins 
	Boat pool with mooring hook
	Happy Hooker (Aaron did this get replaced?)
	Tag Lines
	Tie downs
General mooring inspection (cable, cotters, shackles, lines ...) 
Replace instrument 
	¾” socket
	½” ratchet
	¾” open und wrench
	½” socket
	½” open end wrench
	Tie wraps
Replace instrument batteries 
	½” socket
	½” ratchet
	2 Alkaline DSPL
	Tie wraps
Replace Iridium modem battery 
	½” deep socket
	½” extension
	½” ratchet
	Iridium battery pack
Replace ISUS battery 
	Regular large screw driver
	5/16” socket
	ISUS battery pack
	Gloves
Replace ISUS screen 
	ISUS screen assembly
Clean ISUS sensor tip 
	Tooth Brush
	Alcohol
Inspect bungees (bring spare along)
	Bungee Assembly 
CTD dismount and Replace batteries 
	½” Socket
½” ratchet
½” open end wrench
Large adjustable wrench
9 D-cell alkaline batteries
Unsure what else to get batteries out?
O-Ring set for CTD
Parker O-Ring Lube
Remount CTD Bundle up and strap all cables
	½” Socket
½” ratchet
½” open end wrench
	Tie wraps 
Test communications to instrument 
	Away communications bag
	Radio link to shore
Test communication with CTD 
	Away communications bag
	Radio link to shore
Test communications with ISUS 
	Away communications bag
	Radio link to shore
Recover CTD data and then Clear memory 
	Away communications bag
	Radio link to shore
Recover ISUS data and then clear memory 
	Away communications bag
	Radio link to shore
Confirm CTD and ISUS sample rate is 20 minutes
	Away communications bag
	Radio link to shore
Confirm GPS report received 
	Someone on shore
Take deep breath and think if I missed anything 
	Brain
Deploy refurbished instrument 
	Shoot
	Quick Release
	Cotter Pins
	Pliers
	1-1/8” open end wrench set
	Float
	Dive Bag
Confirm depth and begin mission Go home

Other things
	Cotter pins
	Screw pin shackle
	Howto CTD and ISUS
	Time: 6:30 for 7:00
	Divers: Mike and Mike

