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Bryant,
Key Tasks

· Specifications for 120 psi testing:

Cartridge:

· Check valves


· Must hold 95psi backpressure for 20 minutes

· Cracking pressure must be high enough to seal, but <10psi

· Check valves must be compatible with our chemistry

· Syringes

· Spring return in air syringe is preferred, but syringe must generate 95 psi

· will have threaded return

· throw will be 35mm

· actuation force goal is a delta of 8 lbs

· Cartridge Valve

· Hard stops must place valve in final, sealed position

· Hard stops must hold 20lbs (or 5x minimum stiction)

· Reduce o-ring catch

· Manifold

· Must not leak

Puck

· Must not leak at 120psi

· Must work within new cartridge for functional testing

· No leakage around thin spot

· Must filter at same rate as V1 puck and evacuate same as V4 puck

· We would like to review their test plan

· We would like to attend their functional testing
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