1. Isolation
1.1. Sea-Tox flush selector valve (3-way, pressure neutral, 1mm min port dia, 15psi max differential)
1.1.1. Solenoid
1.1.2. Oil compensated
1.1.3. Multi Port valves
1.2. Bulkhead valves (Seawater, 500 psi, 1mm min port, small scale, low power, size <C- battery, high reliability, overpressure shut-off)
1.2.1. Direct lift solenoid valves
1.2.2. Custom Body valves
1.2.3. Axial flow thru valves
1.2.4. Turn valves
1.2.5. Multi Port valves
1.3. Cartridge Array valves (Seawater, 500 psi, 1mm min port, small scale, low power, size <AAA- battery, flush free valve)
1.3.1. Direct lift solenoid valves
1.3.2. Custom Body valves
1.3.3. Turn valves
1.3.4. Axial pull valves
1.3.5. Dual port single throw valve (eliminates output check valve)
1.4. Cartridge check valves (reliable seal, 500 psid, <5psi opening, any orientation, non-corrosive, small scale <AAA batter)
1.4.1. Spring loaded check
1.5. Sea pressure fittings (500psi, 1mm min thru, non corroding, vibration resistant, and reliable seal)
1.5.1. ¼-28 flat seals 
1.5.1.1. Dibafit
1.5.1.2. Upchurch
1.5.1.3. 

2. Filter 
2.1. 25mm dia (or similar area) filtering media
2.2. 
2.3. Filters integrated in seal mount/chip/cartridge
