General Notes

This calculation was performed with:
Program:	cymex®
Release:	cymex 3.10.4
Edition:	StudioPlus-Edition

This Calculation of a drive system is usable for a rough overview of the usability of gearbox and motor. Especially the motor must be reviewed by the motor manufacturer. 
1	Application: turntable
1.1	Application Data

Parameter	Name	Unit	Value	
eccentric mass	me	[kg]	    10.190	
lever arm for lateral load	x2	[mm]	    25.000	
lever arm for axial load	y2	[mm]	  1000.000	
tilting angle out of horizontal	alpha	[°]	    90.000	
starting angle of movement	fi0	[°]	     0.000	
constant friction torque	Tr	[Nm]	   200.000	
efficiency	eta	[1]	     1.000	
type of motion profile	Typ	[-]	Profiler	
maximum rotational speed	nMax	[1/min]	     1.000	
maximum angular acceleration	aMax	[Rad/s²]	     0.003	
mass moment of inertia (application)	JMax	[kgm²]	     0.480	
process load	TMax	[Nm]	     0.000	
lateral force	QMax	[N]	     0.000	
axial force	AMax	[N]	     0.000	

				

				
1.2	Cycle Data

Parameter	Name	Unit	Value	
Time of movement:	tMov	[s]	  1860.000	
Time of cycle:	tCyc	[s]	  1860.000	
Duty cycle:	ED	[%]	   100.000	
Number of cycles per hour:	n	[1]	     1.935	
Shockfactor:	fs	[1]	     1.000	
Calculation due to:		[-]	continuous operation	

1.3	motion profile

1.4	load

2	Transformations
2.1	Transformation 1 between  Application und Gearbox

Type of Transformation	keine	
Parameter	Name	Unit	Value	
-	-	-	-	
-	-	-	-	
-	-	-	-	
-	-	-	-	
-	-	-	-	
-	-	-	-	
-	-	-	-	
-	-	-	-	
-	-	-	-	
-	-	-	-	

2.2	Transformation 2 between Gearbox and Motor

Type of Transformation	keine	
Parameter	Name	Unit	Value	
-	-	-	-	
-	-	-	-	
-	-	-	-	
-	-	-	-	
-	-	-	-	
-	-	-	-	
-	-	-	-	
-	-	-	-	
-	-	-	-	
-	-	-	-	

3	Gearbox Design

Type of gearbox / Size:	TP025	
Gearbox Variant:	EA-Version	
Label	Unit	Calculated Values	Permitted Values	
Gearbox ratio:	[1]	   220.00	-	
Maximum output torque:	[Nm]	   299.97	   480.00	
Maximum output torque (with shock factor):	[Nm]	   299.97	   480.00	
Nominal output torque:	[Nm]	   200.41	   260.00	
Maximum output cross load :		[N]	   100.08	10000000000.00	
Maximum output axial load:	[N]	     0.00	  4150.00	
Maximum output tilting moment:	[Nm]	    11.33	   413.00	
Maximum input speed:	[rpm]	   220.00	  6000.00	
Nominal input speed:	[rpm]	   216.45	  5100.00	
Lever arm for cross load (x2)	[mm]	    25.00	-	
Lever arm for axial load (y2):	[mm]	  1000.00	-	
Safety factor shaft against fatigue:	[1]	   100.00	-	
Safety factor shaft against material flowing:	[1]	   100.00	-	
Service lifetime of output bearings :	[h]	100000.00	-	
Clumping hub diameter:	[mm]	    -1.00	-	
Gearbox efficiency:	[1]	     0.93	-	
Gearbox mass moment of inertia:	[kgcm²]	     0.01	-	
Mass:	[kg]	     5.58	-	

4	Lambda

Gage	l	
Gage 1  	     0.10	
Gage 2  Application / (Gearbox + Motor):	     0.10	
Gage 3  (Application + Gearbox) / Motor:	     0.12	
Gage 4  	     0.12	

alphagetriebe suggest to use l3 at gage 3. 

5	Adapterplate / Bushing

Name	Unit	Articlecode	
Adapterplate	[-]	have combination checked at alpha	
Square dimesion adapterplate:	[mm]	     0.00	
Width adapterplate:	[mm]	     0.00	
Bushing	[-]	have combination checked at alpha	

6	Motor Design
6.1	Technical Data

Motor manufacturer:	WMC	
Type:	TPMA025-110/220x-320x-BPx-015	
Name:	Unit	Calculates Values	Permitted Values	
Maximum torque:	[Nm]	     1.47	     4.20	
Standstill torque::	[Nm]	     0.98	     1.70	
Rms torque:	[Nm]	     0.98	     1.40	
Maximum speed:	[rpm]	   220.00	  7300.00	
Nominal speed:	[rpm]	   216.45	  5625.00	
Mass moment of inertia:	[kgcm²]	     0.94	-	
Shaft Diameter:	[mm]	     0.00	-	

Please note: Manufacturers do not specify all values. In case of any doubt us the characteristic curves to check the motors usability. 

6.2	Characteristic Curves