Western Flyer Avalan

Version:	1.54.4066	
MAC Address:	00:21:74:02:09:53	
Ethernet:	100 Mbps Full Duplex	
Uptime:	0 days 02h 20:10	
Password: 
         
Need help? Online FAQ available at www.AvaLANWireless.com 
Statistics
Radio RSSI:	-46 dBm	
Radio Block Error Rate:	0.0 %	
Radio Total Packets:	25111	
Radio Failed Packets:	32	
Radio Passed Packets:	25079	
Radio Broadcast Packets:	6271	
Radio Unicast Packets:	18840	
Radio Average TX Size:	67 bytes	
Radio Average RX Size:	95 bytes	
Network Settings
IP Address:	192.168.17.17	
Network Mask:	255.0.0.0	
Default Gateway:	0.0.0.0	
HTTP Port:	80	
Device Information
Device Type:	Access Point	
# of Subscriber IDs Issued:	2	
Current RF Channel:	11	
Connected Subscribers:	1	
RF Connected:	Yes	
Radio Active:	Active	
Product Code:	4	
Radio Version:	3	
Radio Firmware Release:	079	

Version:	1.54.4066	
MAC Address:	00:21:74:02:09:53	
Ethernet:	100 Mbps Full Duplex	
Uptime:	0 days 02h 22:20	

Need help? Online FAQ available at www.AvaLANWireless.com 
Statistics
Radio RSSI:	-45 dBm	
Radio Block Error Rate:	0.0 %	
Radio Total Packets:	25280	
Radio Failed Packets:	32	
Radio Passed Packets:	25248	
Radio Broadcast Packets:	6361	
Radio Unicast Packets:	18919	
Radio Average TX Size:	113 bytes	
Radio Average RX Size:	113 bytes	
Device Information
Device Type:	Access Point	
# of Subscriber IDs Issued:	2	
Current RF Channel:	11	
Connected Subscribers:	1	
RF Connected:	Yes	
Radio Active:	Active	
Product Code:	4	
Radio Version:	3	
Radio Firmware Release:	079	
Device Settings

	Description	Value	
Device	Password:		
RF	Channel:	Use DIP 3-8 selection: 0 (auto channel select mode)
(overrides the current DIP 3-8 selection)	
Network	IP Address:	(#.#.#.#)	
	Network Mask:	(#.#.#.#)	
	Default Gateway:	(#.#.#.#)	
	HTTP Port:	(decimal 1-65535)	

Spectrum Scanner
Automatic Scan Interval:               Scan Rate:     Scan Resolution:     
Display Channel Markers: 
If you cannot see the spectrum scanner graphic above this text, 
please install an SVG plugin for Internet Explorer: SVG Plugin.
MAC Address to Device ID Routing Table

There are 5 devices known to this AP (max: 128) 
Device ID	MAC Address	Packet Count	
0001	00:80:2f:12:0b:fe	1473	
0001	00:90:e8:18:37:c1	2104	
0001	00:21:74:02:09:55	14	
0001	00:d0:69:40:4d:9f	1725	
0001	00:90:e8:17:c6:c8	8435	
Upload New Firmware
& 
Browse for firmware file on local computer: 

Advanced Links
Warning! These links are only for use by advanced users!
Please proceed with caution. 

Version:	1.54.4066	
MAC Address:	00:21:74:02:09:53	
Ethernet:	100 Mbps Full Duplex	
Uptime:	0 days 02h 22:41	

Need help? Online FAQ available at www.AvaLANWireless.com 
Warning! These setting are only for use by advanced users!
Please proceed with caution. 
Device Settings

	Description	Value	
Device:	Type:	Access Point (DIP 1 selection)
Subscriber Unit (override DIP 1 selection)	
	# of Subscriber IDs Issued:	An AP can issue from 1 to 63 SU IDs.
(decimal 1-63)	
Encryption:		Enable User Specified Keys 	
	Network Name (32-bit):	xxxx-xxxx
(hex)	
	Encryption Key (128-bit):	xxxx-xxxx-xxxx-xxxx-xxxx-xxxx-xxxx-xxxx
(hex)	

Reset the Device

buoy Avalan

Version:	1.54.4066	
MAC Address:	00:21:74:02:09:55	
Ethernet:	100 Mbps Full Duplex	
Uptime:	0 days 02h 31:56	
Password: 
         
Need help? Online FAQ available at www.AvaLANWireless.com 
Statistics
Radio RSSI:	-45 dBm	
Radio Block Error Rate:	0.0 %	
Radio Total Packets:	19825	
Radio Failed Packets:	58	
Radio Passed Packets:	19767	
Radio Broadcast Packets:	707	
Radio Unicast Packets:	19118	
Radio Average TX Size:	337 bytes	
Radio Average RX Size:	141 bytes	
Network Settings
IP Address:	192.168.17.18	
Network Mask:	255.0.0.0	
Default Gateway:	0.0.0.0	
HTTP Port:	80	
Device Information
Device Type:	Subscriber Unit	
Subscriber ID:	1	
Current RF Channel:	11	
Connected Subscribers:	1	
RF Connected:	Yes	
Radio Active:	Active	
Product Code:	4	
Radio Version:	3	
Radio Firmware Release:	079	

Version:	1.54.4066	
MAC Address:	00:21:74:02:09:55	
Ethernet:	100 Mbps Full Duplex	
Uptime:	0 days 02h 32:16	

Need help? Online FAQ available at www.AvaLANWireless.com 
Statistics
Radio RSSI:	-43 dBm	
Radio Block Error Rate:	0.0 %	
Radio Total Packets:	20014	
Radio Failed Packets:	59	
Radio Passed Packets:	19955	
Radio Broadcast Packets:	707	
Radio Unicast Packets:	19307	
Radio Average TX Size:	370 bytes	
Radio Average RX Size:	155 bytes	
Device Information
Device Type:	Subscriber Unit	
Subscriber ID:	1	
Current RF Channel:	11	
Connected Subscribers:	1	
RF Connected:	Yes	
Radio Active:	Active	
Product Code:	4	
Radio Version:	3	
Radio Firmware Release:	079	
Device Settings

	Description	Value	
Device	Password:		
RF	Channel:	Use DIP 3-8 selection: 0 (auto channel select mode)
(overrides the current DIP 3-8 selection)	
Network	IP Address:	(#.#.#.#)	
	Network Mask:	(#.#.#.#)	
	Default Gateway:	(#.#.#.#)	
	HTTP Port:	(decimal 1-65535)	

Spectrum Scanner
Automatic Scan Interval:               Scan Rate:     Scan Resolution:     
Display Channel Markers: 
If you cannot see the spectrum scanner graphic above this text, 
please install an SVG plugin for Internet Explorer: SVG Plugin.
MAC Address to Device ID Routing Table

There are devices known to this AP (max: ) 
Device ID	MAC Address	Packet Count	
Upload New Firmware
& 
Browse for firmware file on local computer: 

Advanced Links
Warning! These links are only for use by advanced users!
Please proceed with caution. 

Version:	1.54.4066	
MAC Address:	00:21:74:02:09:55	
Ethernet:	100 Mbps Full Duplex	
Uptime:	0 days 02h 32:33	

Need help? Online FAQ available at www.AvaLANWireless.com 
Warning! These setting are only for use by advanced users!
Please proceed with caution. 
Device Settings

	Description	Value	
Device:	Type:	Access Point (override DIP 1 selection)
Subscriber Unit (DIP 1 selection)	
	Subscriber ID:	Every SU must have a unique ID. Valid IDs are from 1 to 63.
(decimal 1-63)	
Encryption:		Enable User Specified Keys 	
	Network Name (32-bit):	xxxx-xxxx
(hex)	
	Encryption Key (128-bit):	xxxx-xxxx-xxxx-xxxx-xxxx-xxxx-xxxx-xxxx
(hex)	

Reset the Device