***READ ME****

Product: USI07-2105  - USB to RS-232 Interface Cable
Manufacturer:  SeaLevel Systems, Inc.
Web Site Add: http://www.sealevel.com		

Overview:
The Drivers shipped with your USB to RS232 cable are for use with any x86 PC host running Microsoft Windows 95/98/ME/NT/2000/XP.  Currently there is no support for Linux using the SeaLINKTM +232 (P/N 2105) USB to Serial cable. The Linux drivers are in development.  For
more information, visit http://www.ultsol.com/Resources.htm.
 
To program the BDI1000/2000 with a host running Linux, please use the yellow RS232 female
to female cable that was shipped with your BDI unit.

Installation Insrtuctions
Visit http://www.ultsol.com/Resources.htm

Download the latest drivers and extract all the Files into a folder.  Run Setup.exe. Follow the instructions to complete the installation. When prompted, attach the SeaLINK+232 cable to a USB port on your Windows computer. Reboot if prompted.

After you install the drivers, connect the BDI unit to the SeaLINK +232 and proceed with programming the BDI2000. Refer to the BDI User’s Manual for the rest of the installation.