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1. Notes

1.1. The May 13th test may be with a rope and a weight instead of the ESP.  Pressure transducer and/or accelerometer on the buoy.

1.2. The May 17th test should use the ESP and the E\M cable.  PT and accelerometer still on the buoy

1.3. The May 28th test should have the pressure transducer and accelerometer in the ESP housing

2. Deployment/Recover

2.1. Deploy the system, don’t let go

2.1.1. check radio link

2.2. Recover the system

2.3. Deploy the system, let go

2.3.1. check radio link

2.4. Recover the system

3. Initial profiler checkout (no tension control)
3.1. Deploy the system w/no tension control – pure velocity and position

3.1.1. Stay close

3.2. Payout 10 meters at 1 rev/min
3.2.1. cable will be marked and we should be able to check 10 m payout with binoculars

3.3. Payin at 1 rev/min
3.3.1. check cable marks

3.4. Repeat 3.1 – 3.3 3X

3.5. Payout 10 meters, hold depth acquiring eng data for ~15 minutes

3.6. Repeat 3.4 – 3.5 for somewhere between 20 and 40 meters
4. Profiler checkout with tension control

4.1. Payout 30 - 40 meters a 1 m/min

4.2. Hold for 10 minutes

4.3. Payin at 1 m/min

4.4. Repeat 4.1-4.4 3X

5. Profiler checkout with acceleration control

5.1. Same as 4
6. Hold depth mode
6.1. Payout to 30 meters

6.2. Put into hold depth mode

6.3. Hold for 20 minutes

6.4. Payin to 20 meters

6.5. Hold for 20 minutes

6.6. Payin to 10 meters

6.7. Hold for 20 minutes

