Stress analysis of espBase2

Note:

Do not base your design decisions solely on the data presented in this report. Use this information in conjunction with experimental data and practical experience. Field testing is mandatory to validate your final design. Simulation helps you reduce your time-to-market by reducing but not eliminating field tests.
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Description

Summarize the FEM analysis on espBase2

Assumptions

Model Information

	Document Name
	Configuration
	Document Path
	Date Modified

	espBase2
	FEAConfig
	O:\MechDrawings\newFrame\espBase2.SLDASM
	Wed Apr 14 12:48:24 2010

	ESPLiftFramAlum-1
	Default<As Machined>
	O:\MechDrawings\newFrame\ESPLiftFramAlum.SLDPRT
	Wed Apr 14 12:57:02 2010

	emTermination-2
	Default
	O:\MechDrawings\emTermination.SLDPRT
	Tue Apr 13 17:49:53 2010

	espBasePlate-1
	Default
	O:\MechDrawings\newFrame\espBasePlate.SLDPRT
	Tue Apr 13 17:53:32 2010

	formedNoseConeAlum-1/formedSidePlateFB2-1
	
	O:\MechDrawings\newFrame\formedSidePlateFB2.SLDPRT
	Wed Apr 14 12:29:26 2010

	formedNoseConeAlum-1/formedSidePlateFB2-2
	
	O:\MechDrawings\newFrame\formedSidePlateFB2.SLDPRT
	Wed Apr 14 12:29:26 2010

	formedNoseConeAlum-1/formedSidePlateLR2-1
	
	O:\MechDrawings\newFrame\formedSidePlateLR2.SLDPRT
	Wed Apr 14 12:29:26 2010

	formedNoseConeAlum-1/formedSidePlateLR2-3
	
	O:\MechDrawings\newFrame\formedSidePlateLR2.SLDPRT
	Wed Apr 14 12:29:26 2010

	leadBallast-2/leadBallast-1
	Default
	C:\GENE\SWPDMWorking\leadBallast.SLDPRT
	Tue Apr 13 17:40:39 2010

	DSPLBattery-2
	Default
	O:\MechDrawings\newFrame\DSPLBattery.SLDPRT
	Wed Jan 27 17:12:07 2010

	DSPLBattery-1
	Default
	O:\MechDrawings\newFrame\DSPLBattery.SLDPRT
	Wed Jan 27 17:12:07 2010

	Regular FW 0.5-60
	Regular FW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular FW 0.5.sldprt
	Wed Mar 10 13:17:36 2010

	Regular FW 0.5-61
	Regular FW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular FW 0.5.sldprt
	Wed Mar 10 13:17:36 2010

	Regular FW 0.5-62
	Regular FW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular FW 0.5.sldprt
	Wed Mar 10 13:17:36 2010

	Regular FW 0.5-59
	Regular FW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular FW 0.5.sldprt
	Wed Mar 10 13:17:36 2010

	ShallowPressureCase-1
	Default
	X:\ESP\TopLevelAssy\Shallow_Water_Housing_2G\ShallowPressureCase.SLDASM
	Fri Apr 02 17:23:55 2010

	leadBrick-17
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	Regular LW 0.5-48
	Regular LW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular LW 0.5.sldprt
	Wed Mar 10 13:19:59 2010

	HNUT 0.5000-13-D-N-48
	HNUT 0.5000-13-D-N
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\HNUT 0.5000-13-D-N.sldprt
	Wed Mar 10 13:21:55 2010

	Regular LW 0.5-49
	Regular LW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular LW 0.5.sldprt
	Wed Mar 10 13:19:59 2010

	HBOLT 0.5000-13x2x1.25-N-47
	HBOLT 0.5000-13x2x1.25-N
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\HBOLT 0.5000-13x2x1.25-N.SLDPRT
	Thu Mar 25 12:49:06 2010

	HNUT 0.5000-13-D-N-49
	HNUT 0.5000-13-D-N
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\HNUT 0.5000-13-D-N.sldprt
	Wed Mar 10 13:21:55 2010

	Regular FW 0.5-38
	Regular FW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular FW 0.5.sldprt
	Wed Mar 10 13:17:36 2010

	Regular LW 0.5-37
	Regular LW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular LW 0.5.sldprt
	Wed Mar 10 13:19:59 2010

	Regular LW 0.5-36
	Regular LW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular LW 0.5.sldprt
	Wed Mar 10 13:19:59 2010

	Regular FW 0.5-37
	Regular FW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular FW 0.5.sldprt
	Wed Mar 10 13:17:36 2010

	HBOLT 0.5000-13x2x1.25-N-48
	HBOLT 0.5000-13x2x1.25-N
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\HBOLT 0.5000-13x2x1.25-N.SLDPRT
	Thu Mar 25 12:49:06 2010

	Regular FW 0.5-35
	Regular FW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular FW 0.5.sldprt
	Wed Mar 10 13:17:36 2010

	Regular FW 0.5-36
	Regular FW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular FW 0.5.sldprt
	Wed Mar 10 13:17:36 2010

	HNUT 0.5000-13-D-N-36
	HNUT 0.5000-13-D-N
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\HNUT 0.5000-13-D-N.sldprt
	Wed Mar 10 13:21:55 2010

	HBOLT 0.5000-13x2x1.25-N-36
	HBOLT 0.5000-13x2x1.25-N
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\HBOLT 0.5000-13x2x1.25-N.SLDPRT
	Thu Mar 25 12:49:06 2010

	HBOLT 0.5000-13x2x1.25-N-35
	HBOLT 0.5000-13x2x1.25-N
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\HBOLT 0.5000-13x2x1.25-N.SLDPRT
	Thu Mar 25 12:49:06 2010

	HNUT 0.5000-13-D-N-37
	HNUT 0.5000-13-D-N
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\HNUT 0.5000-13-D-N.sldprt
	Wed Mar 10 13:21:55 2010

	HBOLT 0.5000-13x2x1.25-N-45
	HBOLT 0.5000-13x2x1.25-N
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\HBOLT 0.5000-13x2x1.25-N.SLDPRT
	Thu Mar 25 12:49:06 2010

	HBOLT 0.5000-13x2x1.25-N-46
	HBOLT 0.5000-13x2x1.25-N
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\HBOLT 0.5000-13x2x1.25-N.SLDPRT
	Thu Mar 25 12:49:06 2010

	HNUT 0.5000-13-D-N-47
	HNUT 0.5000-13-D-N
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\HNUT 0.5000-13-D-N.sldprt
	Wed Mar 10 13:21:55 2010

	Regular FW 0.5-56
	Regular FW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular FW 0.5.sldprt
	Wed Mar 10 13:17:36 2010

	Regular FW 0.5-58
	Regular FW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular FW 0.5.sldprt
	Wed Mar 10 13:17:36 2010

	Regular FW 0.5-57
	Regular FW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular FW 0.5.sldprt
	Wed Mar 10 13:17:36 2010

	Regular LW 0.5-47
	Regular LW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular LW 0.5.sldprt
	Wed Mar 10 13:19:59 2010

	HNUT 0.5000-13-D-N-46
	HNUT 0.5000-13-D-N
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\HNUT 0.5000-13-D-N.sldprt
	Wed Mar 10 13:21:55 2010

	Regular FW 0.5-55
	Regular FW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular FW 0.5.sldprt
	Wed Mar 10 13:17:36 2010

	Regular LW 0.5-46
	Regular LW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular LW 0.5.sldprt
	Wed Mar 10 13:19:59 2010

	Regular FW 0.5-63
	Regular FW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular FW 0.5.sldprt
	Wed Mar 10 13:17:36 2010

	HBOLT 0.5000-13x2x1.25-N-50
	HBOLT 0.5000-13x2x1.25-N
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\HBOLT 0.5000-13x2x1.25-N.SLDPRT
	Thu Mar 25 12:49:06 2010

	Regular LW 0.5-50
	Regular LW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular LW 0.5.sldprt
	Wed Mar 10 13:19:59 2010

	HNUT 0.5000-13-D-N-50
	HNUT 0.5000-13-D-N
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\HNUT 0.5000-13-D-N.sldprt
	Wed Mar 10 13:21:55 2010

	HBOLT 0.5000-13x2x1.25-N-49
	HBOLT 0.5000-13x2x1.25-N
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\HBOLT 0.5000-13x2x1.25-N.SLDPRT
	Thu Mar 25 12:49:06 2010

	HNUT 0.5000-13-D-N-51
	HNUT 0.5000-13-D-N
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\HNUT 0.5000-13-D-N.sldprt
	Wed Mar 10 13:21:55 2010

	Regular FW 0.5-64
	Regular FW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular FW 0.5.sldprt
	Wed Mar 10 13:17:36 2010

	Regular LW 0.5-51
	Regular LW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular LW 0.5.sldprt
	Wed Mar 10 13:19:59 2010

	leadBrick-46
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-45
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	DSPLBattery-3
	Default
	O:\MechDrawings\newFrame\DSPLBattery.SLDPRT
	Wed Jan 27 17:12:07 2010

	leadBrick-44
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-43
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	Regular FW 0.5-66
	Regular FW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular FW 0.5.sldprt
	Wed Mar 10 13:17:36 2010

	leadBrick-42
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-41
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	ESPSim-1
	Default
	O:\MechDrawings\newFrame\ESPSim.SLDPRT
	Tue Apr 13 14:41:49 2010

	Regular FW 0.5-65
	Regular FW 0.5
	C:\Documents and Settings\magene\My Documents\SWToolboxParts\Regular FW 0.5.sldprt
	Wed Mar 10 13:17:36 2010

	leadBrick-48
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-47
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-50
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-51
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-49
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-54
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-52
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-53
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-56
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-58
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-61
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-62
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-60
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-55
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-59
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-57
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009

	leadBrick-63
	Default
	O:\MechDrawings\leadBrick.SLDPRT
	Wed Oct 14 14:01:29 2009


Study Properties

	Study name
	Study 1

	Analysis type
	Static

	Mesh Type:
	Mixed Mesh

	Solver type
	Automatic

	Inplane Effect: 
	Off

	Soft Spring: 
	On

	Inertial Relief: 
	Off

	Thermal Effect: 
	Input Temperature

	Zero strain temperature
	77.000000

	Units
	Fahrenheit

	Include fluid pressure effects from SolidWorks Flow Simulation
	Off

	Friction: 
	Off

	Ignore clearance for surface contact
	Off

	Use Adaptive Method: 
	Off


Units

	Unit system:
	English (IPS)

	Length/Displacement
	in

	Temperature
	Fahrenheit

	Angular velocity
	Hz

	Stress/Pressure
	psi


Material Properties

Solid Bodies

	No.
	Body Name
	Material
	Mass
	Volume

	1
	ESPLiftFramAlum-1
	[SW]6061-T6 (SS)
	2.80065 kg
	0.00103728 m^3

	2
	ESPLiftFramAlum-1
	[SW]6061-T6 (SS)
	4.94437 kg
	0.00183125 m^3

	3
	ESPLiftFramAlum-1
	[SW]6061-T6 (SS)
	4.94466 kg
	0.00183136 m^3

	4
	ESPLiftFramAlum-1
	[SW]6061-T6 (SS)
	4.9436 kg
	0.00183096 m^3

	5
	ESPLiftFramAlum-1
	[SW]6061-T6 (SS)
	2.80065 kg
	0.00103728 m^3

	6
	ESPLiftFramAlum-1
	[SW]6061-T6 (SS)
	4.94362 kg
	0.00183097 m^3

	7
	ESPLiftFramAlum-1
	6061-T6 (SS)
	4.75304 lb
	48.7273 in^3

	8
	ESPLiftFramAlum-1
	6061-T6 (SS)
	4.75304 lb
	48.7273 in^3

	9
	ESPLiftFramAlum-1
	6061-T6 (SS)
	4.70663 lb
	48.2515 in^3

	10
	emTermination-2
	[SW]6061-T6 (SS)
	0.963011 kg
	0.000356671 m^3

	11
	espBasePlate-1
	[SW]6061-T6 (SS)
	16.7462 kg
	0.00620228 m^3

	12
	formedNoseConeAlum-1/formedSidePlateFB2-1
	[SW]6061-T6 (SS)
	9.49882 kg
	0.00351808 m^3

	13
	formedNoseConeAlum-1/formedSidePlateFB2-2
	[SW]6061-T6 (SS)
	9.49882 kg
	0.00351808 m^3

	14
	formedNoseConeAlum-1/formedSidePlateLR2-1
	[SW]6061-T6 (SS)
	9.62906 kg
	0.00356632 m^3

	15
	formedNoseConeAlum-1/formedSidePlateLR2-3
	[SW]6061-T6 (SS)
	9.62906 kg
	0.00356632 m^3

	16
	leadBallast-2/leadBallast-1
	[SW]Pure Lead
	655.965 kg
	0.0596331 m^3


	Material name:
	[SW]6061-T6 (SS)

	Description:
	

	Material Source:
	

	Material Model Type:
	Plasticity - von Mises

	Default Failure Criterion:
	Unknown

	Application Data:
	


	Property Name
	Value
	Units
	Value Type

	Elastic modulus
	6.9e+010
	N/m^2
	Constant

	Poisson's ratio
	0.33
	NA
	Constant

	Shear modulus
	2.6e+010
	N/m^2
	Constant

	Mass density
	2700
	kg/m^3
	Constant

	Tensile strength
	3.1e+008
	N/m^2
	Constant

	Yield strength
	2.75e+008
	N/m^2
	Constant

	Thermal expansion coefficient
	2.4e-005
	/Kelvin
	Constant

	Thermal conductivity
	166.9
	W/(m.K)
	Constant

	Specific heat
	896
	J/(kg.K)
	Constant

	Hardening factor (0.0-1.0; 0.0=isotropic; 1.0=kinematic)
	0.85
	NA
	Constant


	Material name:
	6061-T6 (SS)

	Description:
	

	Material Source:
	

	Material Model Type:
	Linear Elastic Isotropic

	Default Failure Criterion:
	Max von Mises Stress

	Application Data:
	


	Property Name
	Value
	Units
	Value Type

	Elastic modulus
	1.0008e+007
	psi
	Constant

	Poisson's ratio
	0.33
	NA
	Constant

	Shear modulus
	3.771e+006
	psi
	Constant

	Mass density
	0.097544
	lb/in^3
	Constant

	Tensile strength
	44962
	psi
	Constant

	Yield strength
	39885
	psi
	Constant

	Thermal expansion coefficient
	1.3333e-005
	/Fahrenheit
	Constant

	Thermal conductivity
	0.0022322
	BTU/(in.s.F)
	Constant

	Specific heat
	0.21405
	Btu/(lb.F)
	Constant

	Hardening factor (0.0-1.0; 0.0=isotropic; 1.0=kinematic)
	0.85
	NA
	Constant


	Material name:
	[SW]Pure Lead

	Description:
	

	Material Source:
	

	Material Model Type:
	Linear Elastic Isotropic

	Default Failure Criterion:
	Unknown

	Application Data:
	


	Property Name
	Value
	Units
	Value Type

	Elastic modulus
	1.4e+010
	N/m^2
	Constant

	Poisson's ratio
	0.4
	NA
	Constant

	Shear modulus
	4.9e+010
	N/m^2
	Constant

	Mass density
	11000
	kg/m^3
	Constant

	Thermal expansion coefficient
	5.3e-005
	/Kelvin
	Constant

	Thermal conductivity
	35
	W/(m.K)
	Constant

	Specific heat
	130
	J/(kg.K)
	Constant


Loads and Restraints

Fixture

	Restraint name
	Selection set
	Description

	Fixture-23 <emTermination-2>
	 on 1 Face(s) fixed.
	 

	Fixture-24 <espBasePlate-1>
	 on 1 Face(s) with respect to reference geometry Top Plane with  displacement 0.000000 in rotation 0.000000 rad along plane  Dir 1  displacement 0.000000 in rotation 0.000000 rad along plane  Dir 2
	 


Load

	Load name
	Selection set
	Loading type
	Description

	Gravity-1
	Gravity with respect to Top Plane with gravity acceleration -773 in/s^2 normal to reference plane 
	Sequential Loading
	 


Connector Definitions

               No Connectors were defined

Contact

Contact state: Touching faces - Bonded

	Contact Set-169
	Between selected entities of ESPLiftFramAlum-1 and formedNoseConeAlum-1/formedSidePlateLR2-1

	Description:
	 

	Contact Set-170
	Between selected entities of ESPLiftFramAlum-1 and formedNoseConeAlum-1/formedSidePlateLR2-3

	Description:
	 

	Contact Set-260
	Between selected entities of ESPLiftFramAlum-1 and espBasePlate-1

	Description:
	 

	Contact Set-261
	Between selected entities of ESPLiftFramAlum-1 and espBasePlate-1

	Description:
	 

	Contact Set-288
	Between selected entities of ESPLiftFramAlum-1 and ESPLiftFramAlum-1

	Description:
	 

	Contact Set-289
	Between selected entities of ESPLiftFramAlum-1 and ESPLiftFramAlum-1

	Description:
	 

	Contact Set-294
	Bonded contact pair: Between selected entities of emTermination-2 and ESPLiftFramAlum-1

	Description:
	 


Mesh Information

	Mesh Type:
	Mixed Mesh

	Mesher Used: 
	Standard mesh

	Automatic Transition: 
	Off

	Smooth Surface: 
	On

	Jacobian Check: 
	4 Points 

	Element Size:
	1.2 in

	Tolerance:
	0.06 in

	Quality:
	High

	Number of elements:
	22961

	Number of nodes:
	39392

	Time to complete mesh(hh;mm;ss): 
	00:00:21

	Computer name: 
	SANTORINI


Design Scenario Results

        No data available.

Sensor Results

        No data available.

Reaction Forces

	Selection set
	Units
	Sum X
	Sum Y
	Sum Z
	Resultant

	Entire Body
	lb
	5.25267e-005
	3285.89
	0.000913749
	3285.89


Reaction Moments

	Selection set
	Units
	Sum X
	Sum Y
	Sum Z
	Resultant

	Entire Body
	lb-in
	0
	0
	0
	8.85075e-033


Free-Body Forces

        Free Body Forces not available.

Bolt Forces

        No data available.

Pin Forces

        No data available.

Study Results

Default Results
	Name
	Type
	Min
	Location
	Max
	Location

	Stress1
	TXY: Shear in Y Dir. on YZ Plane
	0 psi

Element: 22950
	(-14.9364 in,

69.0038 in,

2.17369 in)
	4745.23 psi

Element: 22837
	(4.78005 in,

69.2759 in,

-3.3673 in)

	Stress2
	VON: von Mises Stress
	0 psi

Node: 39091
	(14.936 in,

69.261 in,

3.36717 in)
	11235.6 psi

Node: 244
	(-4.00075 in,

69.1394 in,

2.9466 in)

	Stress3
	VON: von Mises Stress
	0 psi

Node: 39091
	(14.936 in,

69.261 in,

3.36717 in)
	11235.6 psi

Node: 244
	(-4.00075 in,

69.1394 in,

2.9466 in)

	Displacement1
	URES: Resultant Displacement
	0 in

Node: 3134
	(-0.132423 in,

76.9134 in,

0.229363 in)
	0.0252603 in

Node: 34488
	(-15.376 in,

18.3511 in,

-15.6261 in)

	Strain1
	ESTRN: Equivalent Strain
	0 

Element: 22664
	(14.3386 in,

69.262 in,

3.36711 in)
	0.000394639 

Element: 495
	(-3.9061 in,

68.5878 in,

-2.86181 in)
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Conclusion

