Stress analysis of motorMount002

Note:

Do not base your design decisions solely on the data presented in this report. Use this information in conjunction with experimental data and practical experience. Field testing is mandatory to validate your final design. Simulation helps you reduce your time-to-market by reducing but not eliminating field tests.
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Description

Summarize the FEM analysis on motorMount002

Assumptions

Model Information

	Document Name
	Configuration
	Document Path
	Date Modified

	motorMount002
	Default
	O:\MechDrawings\newFrame\motorMount002.SLDPRT
	Wed Dec 23 17:43:27 2009


Study Properties

	Study name
	Study 1

	Analysis type
	Static

	Mesh Type:
	Solid Mesh

	Solver type
	FFEPlus

	Inplane Effect: 
	Off

	Soft Spring: 
	Off

	Inertial Relief: 
	Off

	Thermal Effect: 
	Input Temperature

	Zero strain temperature
	298.000000

	Units
	Kelvin

	Include fluid pressure effects from SolidWorks Flow Simulation
	Off

	Friction: 
	Off

	Ignore clearance for surface contact
	Off

	Use Adaptive Method: 
	Off


Units

	Unit system:
	English (IPS)

	Length/Displacement
	in

	Temperature
	Fahrenheit

	Angular velocity
	Hz

	Stress/Pressure
	psi


Material Properties

	No.
	Body Name
	Material
	Mass
	Volume

	1
	motorMount002
	[SW]5052-H32
	17.6636 kg
	0.00659088 m^3

	2
	motorMount002
	[SW]5052-H32
	2.63504 kg
	0.000983224 m^3

	3
	motorMount002
	[SW]5052-H32
	2.63504 kg
	0.000983224 m^3


	Material name:
	[SW]5052-H32

	Description:
	

	Material Source:
	

	Material Model Type:
	Linear Elastic Isotropic

	Default Failure Criterion:
	Unknown

	Application Data:
	


	Property Name
	Value
	Units
	Value Type

	Elastic modulus
	7e+010
	N/m^2
	Constant

	Poisson's ratio
	0.33
	NA
	Constant

	Shear modulus
	2.59e+010
	N/m^2
	Constant

	Mass density
	2680
	kg/m^3
	Constant

	Tensile strength
	2.3e+008
	N/m^2
	Constant

	Yield strength
	1.95e+008
	N/m^2
	Constant

	Thermal expansion coefficient
	2.4e-005
	/Kelvin
	Constant

	Thermal conductivity
	137
	W/(m.K)
	Constant

	Specific heat
	880
	J/(kg.K)
	Constant


Loads and Restraints

Fixture

	Restraint name
	Selection set
	Description

	Fixture-5 <motorMount002>
	 on 4 Edge(s) fixed.
	 


Load

	Load name
	Selection set
	Loading type
	Description

	Force/Torque-1 <motorMount002>
	 on 1 Face(s) apply  force 5000 lb  normal to reference plane  with respect to selected reference Edge< 1 > using uniform distribution 
	Sequential Loading
	


Connector Definitions

               No Connectors were defined

Contact

Contact state: Touching faces - Bonded

Mesh Information

	Mesh Type:
	Solid Mesh

	Mesher Used: 
	Standard mesh

	Automatic Transition: 
	Off

	Smooth Surface: 
	On

	Jacobian Check: 
	4 Points 

	Element Size:
	1.1325 in

	Tolerance:
	0.056624 in

	Quality:
	High

	Number of elements:
	10291

	Number of nodes:
	20679

	Time to complete mesh(hh;mm;ss): 
	00:00:06

	Computer name: 
	SANTORINI


Design Scenario Results

        No data available.

Sensor Results

        No data available.

Reaction Forces

	Selection set
	Units
	Sum X
	Sum Y
	Sum Z
	Resultant

	Entire Body
	lb
	0.0295281
	4999.89
	0.330445
	4999.89


Free-Body Forces

	Selection set
	Units
	Sum X
	Sum Y
	Sum Z
	Resultant

	Entire Body
	lb
	0.00199563
	0.00257561
	0.000487918
	0.0032946


Free-body Moments

	Selection set
	Units
	Sum X
	Sum Y
	Sum Z
	Resultant

	Entire Body
	lb-in
	0
	0
	0
	8.85075e-033


Bolt Forces

        No data available.

Pin Forces

        No data available.

Study Results

Default Results
	Name
	Type
	Min
	Location
	Max
	Location

	Stress1
	VON: von Mises Stress
	34.1148 psi

Node: 1017
	(1.2726 in,

-3.06293 in,

0.0131407 in)
	52082.6 psi

Node: 18217
	(16 in,

-12.25 in,

-12.75 in)

	Displacement1
	URES: Resultant Displacement
	0 in

Node: 28
	(-16 in,

-12.25 in,

-10.75 in)
	0.195271 in

Node: 224
	(3.02608 in,

2.80016 in,

-0.00133002 in)

	Strain1
	ESTRN: Equivalent Strain
	7.19148e-006 

Element: 1094
	(1.58473 in,

-3.44525 in,

-0.0555275 in)
	0.00186757 

Element: 8239
	(15.7404 in,

-12.1936 in,

12.4294 in)
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