Windows NT to VxWorks SLIP Connection Setup





New Modem Installation





     1)  Install the VxWorksSLIP.inf file into the \Winnt\Inf\ directory





     2)  Click  Start-> Settings-> Control Panel-> Modems 





     3) Click ADD, check Don't detect my modem...  and click  Next 





     4)  In the  Install New Modem  window, click on  (NULL Modem Types )


          under Manufacturers and VxWorks SLIP NULL Modem under Models.


          Click Next.


 


     5)  Click Selected ports-> COMx-> Next  (choose a Com port)





     6)  Click Finish to complete the New Modem installation. 





     7)  In the Modem Properties window, highlight VxWorks SLIP NULL Modem


           and click Properties.  





      8)  Under the General tab, set  Maximum Speed to 115200 





      9) Under Connection, set Connection preferences to 8, None, 1





    10)  Click Advanced, uncheck Use flow control and click OK.





    11) Click OK and Close to finish the modem setup.


 


    12)  A window should pop up with the request: Dial-up Networking needs...Would you like


           to do this now?  Click Yes.





    13)  When the Remote Access Setup window appears, click Add and select Com1-


            VxWorks SLIP NULL Modem under RAS-Capable Devices. 





    14) Click OK->Continue.





    15) Click Yes to reboot when the Network settings changed....  message appears.





 


Dial-Up Networking Setup 





    1)  Click  Start-> Programs-> Accessories-> Dial-Up Networking	





    2)  Click New, enter a  phonebook entry name and click Next. 





    3)  Uncheck all boxes under Server and click Next. 





    4)  Select VxWorks...., Next-> Next-> Finish.





    5)  You should now be back at the Dial-Up Networking window. Select


         your new Phonebook entry and click More followed by Edit entry....





    6)  Select the Server tab and  SLIP: Internet under Dial-up server type: .





    7)  Under Network protocols, check  the TCP/IP box and click on the 


         TCP/IP Settings button.





    8)  Enter the client IP address 128.114.63.71 for the IP address and uncheck both Force IP header  compression and Use default gateway on remote network.





    9)  Click OK-> OK-> Dial -> OK (No User name or Password is needed)





   10) A message box will be generated once a connection is established. 





