   USERS   OF  BEAD   BLASTER

1. DO NOT RUN IF PLASTIC PROTECTIVE COVER IS MISSING FROM UNDERSIDE OF WINDOW.

2. IF COVER IS MISSING OR  TOO SCRATCHED UP,  ASK FOR A NEW ONE FROM THE SHOP OR FROM JIM SCHOLFIELD.

3. CHECK AIR PRESSURE,  IT SHOULD BE ABOUT  80 PSI.

4. DO NOT BLAST OILY,  WET PARTS OR SURFACES.    BLASTER WORKS BEST TO REMOVE DRY, CLEAN CORROSION,  RUST,  OLD PAINT.

5. BE AWARE PLASTIC PARTS CAN BUILD UP A STATIC ELECTRICAL CHARGE.

6. CONTACT SHOP OR JIM SCHOLFIELD ABOUT ANY MALFUNCTION OR  QUESTIONS .

