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        PARTS   LIST   FOR   OVERHEAD  TROLLEY   HOIST  -   AUV   AREA

1. I- Beam  - 4” min. beam height,  2.75-4”wide tapered flange,  for trolley, 

2. Wedge Stud Anchors – 316 S.S.-  3/8”Dia.,  3.375” embedded length,  OR as specified.

3. Hoist –– 2 hoists on common beam.  NOTE:  hoists will each be placarded, 500 lbs. Max.  

a. CM Loadstar, manual trolley mount,  1000lb. Cap., 8 fpm,  10 ft. lift, $1767.48

b. CM Loadstar,  man. Trolley mt, 1000lb. Cap., 16 fpm with creep mode for accurate positioning, 10 ft lift,  $2517.12

4. Push Trolley – CM 632, low head room, 4 roller,  1000 lb. Cap.,  $106.19

5.
Misc. – chain containers, electrical cord festoon trolleys,  other hardware for mounting beam.

