              PRESSURE    TEST    RECORD

Test Date:  

Item Description :  

Item S/N:  

Tested For: MBARI at our own Pressure Test Facilities- Large Chamber
Test Pressure:  

  xxxx  psi / 1.5 S.F = xxxx psi     xxxx / 1.487 psi/meter S.W. = xxxx meters water depth.
Gauge:  Heise Dial
Gauge S/N:  H35771
Gauge Range:  0-10000 psi

Calibration Date:  8/30/06  with a PSI-Tronixs 0-10ksi digital gage, PG-5000, S/N K0637. This unit calibrated 7/27/06, 0-10ksi +/- 0.1%FS, to ANSI / NCSL Z540.1 standards by Scientific Technologies Inc. with an AMETEK DWT, Cert.# 402503  

The test articles were subjected to the implodable items alternative procedure stipulating 10 cycles to maximum allowed pressure.  A 1 minute hold at 0 and xxxx psi on cycles 
1-9 and a 60 minute hold at xxxx psi on the 10th cycle. 
 No evidence of leaks or damage was noted.  
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