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                Pressure Facility Refurbishment/Modification,  MBARI


                                        “The Bullet”











Paul, Troy,         Here’s an updated list of what we want done.  We can adjust P.O. as required for the small additional tasks I have included.








Sandblast inside and outside surfaces.





Bore and thread 3,  3/8-16 holes in lid as indicated.





Plug/fill-weld indicated Port on lid  for pressure integrity and smooth resulting surface.





Recut “O”ring groove as indicated/discussed in projectile body.  Note included spec’s for O’ring grooves.  Lid and body O’ring  mating surfaces need to be metal/metal fit, flat and parallel to +- 0.002and a -32 surface finish.





Paint all exterior surfaces with durable white epoxy paint.








     Questions- 408-775-1765                             Thanks,     





                                                                                              Jim Scholfield








