                                                                                                                        11/17/06

Desert Star Systems,  LLC
RE: Sharkeye II Pressure tests

Jesse,  Please find enclosed the test results.  No pressure test  damage or leaks were noted except residual marks on the sealing surface of the cast acrylic cap mainly from the o’ring.  These marks were expected due to the nature of the material and the pressures encountered.  Both tests were 2 cycles  0 – 5880 psi,, hold 1 minute, return to 0. The 3rd cycle included a 60 minute soak at 5880 psi.  Maximum rate was 1000 psi/min.
You will find residual mineral oil in crevices and holes.  I washed most off using warm soapy water.  

I again apologize for the cosmetic damage on the aluminum cap and the inner edge of the housing.  I had carefully filed out a very slight raised section on both which could have interfered with a proper seal at some future time.  The lid was slippery with oil and slid out of my hand when I was getting ready to clean the parts.  NUTS.    

An invoice I prepared showed a total of $808.00.   You should see it in 10 days or so.  

Nice product.  Thanks,  

                                           Jim Scholfield

                                           scji@mbari.org
                                           831-775-1765

