FOCE  FLUME  CORE  FASTENER  CALL-OUT                            9/31/08                      



-¼-20 unless otherwise stated, Nylok Nuts,  washers


-SS 316 where possible

30  
10-32 x 1.25” pan head 
Polycarbonate joints – (Barrel Nuts)  

36
4” FHS


Polycarb. Side mts. (1” stand-off)

24
3 ½”  FHS  thru Rein. Plates
Polycarb. Top mts.

16
3”  FHS   thru FRP only
Polycarb. Top mts.


78
2 ¾” HHCS


Reinf. Plates,  side 
40
2 ¾” HHCS


Reinf. Plates,  top

16
5”  HHCS


FRP to FRP thru top reinf. plates
4
4 ½ “ FHS


Clevis

8
2 ½ “ HHCS


Clevis

4
½ -13 x 5” HHCS

Clevis Pins


56
10-24 x 1” FHSS

motor/fan polycarb. Inner Mts
24
10-24 x 1” SHCS 

motor/fan polycarb. Outside Mts

24
3 ½ “ SHCS


fan pulley shaft mts

8
10- 24 x 3 ½ “ SHCS

motor mts
40
¾” NYLON SHCS

Hex Screen frames
8
½” -13  NYLON Nuts

Hex Screen Support rods

16
3”   HHCS


SS Latch Brackets
2
3”  3/8 X 16 HHCS

Latch Pivot Bolts

24
3”  HHCS


FRP Wing Support Doubled Stiffeners

38
2 ¾” HHCS 


FRP Wing Support Stiffeners

TOTAL - ~500 + appropriate washers and nuts (Nylok)

