Maxon Fan Drive- belts  and Elmo controller    

Power Usage @ 300 cts/sec 

AC Amps reported

W/Dtrain @ 4 deg C.

4.75

W/Dtrain @ 10 deg C.
2.8

WO/Dtrain@4 deg C.

1.37

W/DTrain WO oil

1.5

 W/DTrain in Air

2.8

W/WO Drive Train and Water (belts)4 deg. C
4.75 – 1.37 = 3.38 AC Amps

Drive Train and water(belts)10 vs. 4 deg

4.75 – 2.8 = 1.95 

W/WO Drive train in Air



2.8 – 1.37 = 1.43

W/WO oil W/Drive train



2.8 – 1.5 = 1.3

Drive Train W/WO Water @10 deg C

2.8 – 2.8 = 0

Belts have a slightly higher friction load than chains but this shows  oil comping  of motor 
adds 1.3 AC amps
Water load is minimal

