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Gain must be adjusted to account for the Gage Factor of actual gages used.





Adj. Gain until Shunt Cal = 2.0 (1000)/ GF of actual gages





Eg.  Real GF = 2.14        so         Shunt cal needs to be  2.0(1000)/2.14= 934





Adjusted Gain will be 4.67 





(Amp is set to 1000 u   shunt i
