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LRAUV NEW OIL PRESSURE COMP UNIT
1. Procure - Custom top piece with 2 – UpChurch ¼-28 ports plus 4 x 6-32 x 1.25 Fl Head screws,  Fast or Reg. Cure 3M 5200 and 1 x 2-212 Oring
2. Punch 4 holes for 4-40 x 1” SHCP screws and center screw in Bellofram
3. Dry assemble to confirm fitment, bellofram fabric  (piston) side down, 3” 4-40s not used.
4. Abrade – rough sand paper- all delrin parts,  piston, piston top , and housing parts which seal to the Bellofram
5. Clean with all parts with acetone
6.  Apply a very thin film of 3M 5200 to all delrin sealing surfaces,  clean-off radiused bore edge.   	
7. Assemble within 20 minutes if using fast cure.	
8. Let cure for 24 hrs/3 days
9. Trim excess diaphragm and gently install long position indicator into bottom of piston
10. Assemble adaptor/connector top with 2-212 Oring									

