List of MSDS for B138 Mech lab and B103 Tank lab					11/3/16
PRODUCT				TYPE			QUANTITY		
                NOTE: B138 HAS A SNORKLE WHICH IS USED IN CONJUNCTION WITH A VACUUM PUMP SYSTEM, HOWEVER IS RARELY USED WHEN CHEMICAL MIXING SINCE MOST CHEMICALS ARE USED IN SMALL QUANTITIES OR ARE OF LOW VOLITILITY.   IT IS USED, OF COURSE, WITH STRONG VAPORS, ETC.
B138  
BJB PC-10 A, B, C			URETHANE		7 GAL
BJB TC 854				URETHANE		4 GAL	
DUOSEAL VACUUM PUMP OIL		OIL			2 PT
E-PAINT  SN-1				EPOXY PAINT		1 GAL
FISHER METHYLENE CHLORIDE		SOLVENT		1 pt
FLEXANE 94				URETHANE		0.5 GAL
IPS WELD-ON 4				SOLVENT		1 PT
LPS-1 OIL				OIL			1 GAL
MOLD STAR 15				SILICON			5GAL
OMEGA A1011 ARMOR COAT		PAINT			2 CANS
OMEGAA1074 C & G CLEAR		RTV			4 TUBES
OMEGA A1127 LITHO GREASE		GREASE			3 CANS
OMEGA A1044 PROTECT-ALL		PAINT			2 CANS
PLASTIDIP				RUBBER		2 CANS
PMC 770				URETHANE		1 PT
PMC	780				URETHANE		1 PT
[bookmark: _GoBack]3M RESIN PRIMER 5131N		SOLVENT		1 PT
SANCHEM COSMOLENE			GREASE			1 GAL
SCOTCHCAST 2131			URETHANE		3 PACKS
SHELL TELLUS T15			OIL			7 GAL
											P2
SHELL TELLUS T22			OIL			3 GAL
SMOOTHSIL 950			SILICON			0.5 GAL
SMOOTH-ON SORTA-CLEAR 40		SILICON			1 GAL
SMOOTH-ON CRYSTAL CLEAR 204	URETHANE		10 GAL
SMOOTH-ON CRYSTAL CLEAR 220	URETHANE		2 GAL
SMOOTH-ON EPOXACAST 690		EPOXY			2 GAL
SMOOTH-ON FEATHERLITE		EPOXY			1.5 GAL
SMOOTH-ON FOAMIT-10 SLOW		URETHANE		1 GAL
SMOOTH-ON URECOAT			URETHANE		1 GAL
SPRAY PAINT, VARIOUS			PAINT			20 CANS
SLX DENATURED ALCOHOL		SOLVENT		0.5 GAL
SUNNYSIDE ACETONE			SOLVENT		2 GAL
VYTAFLEX 60				RUBBER		1 PT
WASTE OIL				OIL			3 GAL
WELD-ON P-70 PRIMER			SOLVENT		1 GAL
WELD-ON 2711 CEMENT		SOLVENT		1 GAL
XTC-3D					EPOXY			0.5 GAL


B103
CHEVRON LUBE OIL FM			MINERAL OIL		30 GAL
HPU OIL (probably) TELLUS T32		OIL			15 GAL





















