                                                   MOOS Solar Panel Seal                                                                  9/05/03

We are looking for a compliant u-channel extrusion to weather-seal the edge of an aluminum panel in an exposed marine environment.  The seal material needs to have a working life of 10 yrs. in a fully exposed UV/Sunlight condition.  Inside Dim's of 1.00" deep and 1" legs with the legs preferably tapered toward ends.  We intend to glue this seal on.  .125-.25" thick material is fine.  We're looking at 250 ft., maybe more.  Please advise on suitable materials and rough quotes.  Thanks,    Jim

