NOTES ABOUT KECK BB AND SHORT PERIOD SEISMOMETERS AND BATT’S              2/10/04

PARTS- most in McGill,  SW            (EACH BALL)

Mt Plate, Sup’t ring and segments  are water jetted

1. MT Plate-generalized for short period, BB, and batts

2. Support Ring-generalized for 1,2,3,4 penetrations and 180 deg.  for mounting plate

3. 1/8” gum (foam) rubber (soft – Shore 00) McM 8570K19 or 8601K11

-1 x 8” with 2 x ½” holes 4” C/C

-2 x 10.5” with 8 x ½” slot

4.
4 X segments of circle to locate batts, 5.5,6.5”R   7” long

5.
Loctite E-30CL to bond ring to glass,    sanded and cleaned

6. Loctite E-00 or 05 to bond segments to plate-fast set.

7. Styrofoam or rubber to separate  batts

8. 2 x 3/8 - 16 x 12.5” fiberglass threaded rod

9. 4 x ¼-20 hex drive inserts for ring, McM P/N 92105 A100

10. 2 x 3/8-16 hex drive insert for plate, McM P/N 92105 A420

11. delrin 1.5/2” stock, parted ~.4”, to make nuts (4) for thr. Rod, tapped 3/8-16.

12. 2-data logger brackets, start with 1.25 x 1.25 x .125” Angle stock

13. 2 SETS, (4) disk drive brkts,  1.5 x 1 x .062” Angle ?Orchard?) or 5052 flat stock

14. sml batt. Brkts, 4 for each data logger .   

15. Big batt upper plate, 8”Dia. 2 holes, Make from inside of Sup’t rings

