              PRESSURE    TEST    RECORD

Test Date:  7/28/06
Item Description:


MODEL


S/N



Acoustic Modem
ATM-887


1107
Tested For: MBARI at our own Pressure Test Facilities
Test Pressure:  8800 psi
 Gauge:  
Gauge 1 – Heise- Dial


Gauge 2 – Enerpac -dial

Gauge S/N:  

H35771



none
Calibration Date:  
9/15/97 ; +- 20 psi


New – out of the box



(in continuous use to present)

+- ½ % F.S. 
Gauge Range:  Both - 0-10,000 psi     - NOTE:  I ran these gauges in parallel realizing an 8 year old cal. on the Heise would not be totally satisfactory.  The gauges agreed on all readings to within 0.4%.  My transfer standard Digital gage was out for service but I believe you will find my alternative method very satisfactory to your requirements.  
Procedure:

The test articles were subjected to the implodable items alternative procedure stipulating 10 cycles to maximum allowed pressure.  A 1 minute hold at 0 and 8800 psi on cycles 
1-9 and a 60 minute hold at 8800 psi on the 10th cycle. 
 Results: 

8800 psi / 1.5 S.F. = 5867 psi     5867 / 1.487 psi/meter S.W. = 3945 meters S.W.


No evidence of leaks or damage was noted.  

Test Technician:   




James T. Scholfield



831-775-1765




MBARI




scji@mbari.org



7700 Sandholdt Rd.




Moss Landing, CA.  95039

