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REMOVAL OF PROPS AND MOTORS





	PROPS


	1. remove hub (1/2 “ nylok nut and washer)


		- unscrew all thread (1/2” short wrench)


		- unscrew large prop retaining nut (15/16” socket and piece of wood to block prop)


	


	2. using prop removal tool - carefully loosen prop from tapered shaft (9/16”)


		- woodruff key should stay with shaft





	MOTOR 


	1. disconnect compensation and electrical connectors - pay attention to both internal and external 		    “O” rings,  put protective caps on open connectors if possible


	


	2.  remove fairing/bracket over wiring if necessary (7/16”)


		-make sure the wiring bundle is free to be removed with the motor





	3. crack loose 4 allen bolts holding motor - remove 3 lowest ones assuring that the remaining bolt 		    holds the motor securely; i.e. the motor does not sag and bend the remaining bolt. (5/16” allen)


	


	4. make sure other equipment/wiring is out of danger of being damaged. 


		NOTE: Motor is heavy and slippery (50 + LBS), and the connectors are awkward . 


		- station another person to support the motor


		- remove last allen bolt to release the motor








INSTALLATION OF PROPS AND MOTORS - Installation is the reverse of removal except:





	1. use cop
