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Tethys VB Pump Repair – 11/12/10

The driven magnet had come loose from the pump shaft.  A structural multi-surface epoxy was used to bond the magnet back onto the shaft.  After curing, pump was reassembled and tested.  A 12.4 VDC supply was set to 3.0Amps Max.,  oil was pumped thru a valve to simulate back pressure.
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