During final assembly 2Mohm bleeder resistors were added across the 375V capacitors to provide a slow discharge for safety.

MFG: Vishay
PN: VR37000002004JR500
These are through-hole 0.5W metal film resistors.

At 375V they are dissipating ~70mW (of 500mW rating).

The bulk capacitors are:
· MFG: Kyocera AVX
· PN: FFVE6B0147KJE
· 140uF 800V


They are expected to discharge at roughly the following rate using the t=RC time constant of ~280 seconds.
· 1RC (4.6 minutes)
· 138V
· 2RC (9.3 minutes)
· 50.6V
· 3RC (14 minutes)
· 18.75V
· 4RC (18.6 minutes)
· 6.9V
· 5RC (23.3 minutes)
· 2.25V

This resistor is placed directly across the capacitors leads.
