MARS EOI Seawater Return Measurements 2012
Equipment used:  AMPROBE Ground Probe GP-1
Test performed:  Test C – 3 Point Test

Test configuration:

