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Bus in is 18-36 VDC at 20 Amps peak from Battery

Bus in is 18-36 VDC at 20 Amps peak from Tether

Raw Bus out 18-36 VDC for:


15A:
Tail

1A:
LBL

2A:
Acoustic Modem

0.5A:
Novatech

2A:
DVL

2A:
Spare

2A:
Spare

Isolated DC->DC for:

5V 4A:
PC/104(10/17W) PowerOne IES020YG-A

CPU(4.25/8.5W), Serial(1/2W), CAN(0.5/0.6W), Fan(2W), HD(0.9/2.7W), Hub(1.25W)

Spare(5V)

12V 2.5A:
Components(7/22W) Traco TEN-30

GPS(1/5W), Crossbow (4/4W), Hub (1.5/4W), Acoustic Release (0/1W), RF Modem (0.5/8W)

Spare(12V)

12V 0.1A:
Parosci(0.2W)

Current sense to measure tail

Pressure/Humidity/Temp sensors

Caps, Filters

Reverse Bias Diodes

Positronic Connectors (Removable)

