MARS Prelim instrument checklist

Inspect mechanical
   tight bolts
   housings tight
   strain relief tether
With power off, put in tank
   Run MARS PMACS CONSOLE.exe
      Science Nodes
         External Loads
         allow system to scan for ground faults
Prepare scope to capture inrush current
Turn on power
If inrush too high, insert resistor in power path
Resistor will need to go in the client's housings
Verify network communications

