MBARI MARS HV Risk Assessment
24 March 2010

Set-up Lab HV

Current                   

Action Before Use
Emergency –no number
Emergency contact numbers will be placed on the wall inside the lab.  Eye wash will be provided. 

Open Lab
Close off and create screened area and latch roll-up doors.

Unrestricted Personnel
Access to screened area will be restricted to Alcatel personnel only.

HV Emergency
One MBARI employee, outside screened off area within lab capable of operating AC disconnect, at all times. 

HV Testing

Unrestricted Personnel
Access to screened area will be restricted to Tony Evans.
HV Emergency
One MBARI employee, outside screened off area within lab capable of operating AC disconnect, at all times. 


Fluorinert Fill

Fluorinert Spill
Spill kit, boom, and mats will be set up prior to fluorinert fill.  Drum and plastic bags for waste will be placed outside of lab prior to fill. 

Trip Hazard
Spill kits will be removed before HV testing. 

Fluorinert Drain
Fluorinert Spill
Spill kit, boom, and mats will be set up for fluorinert drainage. 
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             MBARI Safety Representative


           Date

Example Only
Sign off

H&S Officer, HV Specialist, Chemical Advisor?
	Operation
	Risk
	No of People
	Severity
	Likelihood
	Likelihood X Severity
	Action
	Severity
	Likelihood
	Total After Action
	Notes

	Electrical  Test
	High Voltage
	4
	5
	5
	25
	Restrict access, screen area to 1 person operation and 1 person dead switch operation. 
Interlock required within caged area 
HV training required
	5
	1
	5
	Review every six months


Severity
5 Danger of Death

4 Loss of Limb –Severe disablement
3 Major Injury – broken limb etc
2 Minor Injury – cuts, bruises etc

1 no injury
Likelihood

5 Highly likely

4 Probable

3 Possible

2 Not likely 

1 Highly unlikely
Review ‘total after action’ every 6 months if above 4
